|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Sl. no. | Vol no. / Pg no. /Clause no. | Description of clause | Bidders observation |  |
| 1. | Vol No. I commercial Part 2 BEC Pg 24, 25.  1.6 a) | The Leader of the consortium shall satisfy the minimum experience requirement as per Para 1.0 above. | Please delete this clause as it is in contradiction with clause 1.4, which states “Either the Leader or the Member of the Consortium shall have to meet the requirement of Para 1.1 to 1.3 above”. | Being informed through subsequent corringendum. |
| 2. | Vol no. II Process Design Basis.  Pg No. 75 Clause No.2 | M.P Gas outlet temperature= 27 C  L.P Gas outlet temperature = 40 C | Ambient air shall be used for cooling and based on practical utilization of an air-cooled fin fan heat exchanger; it’s not possible to achieve ambient temperature at the exit of after cooler.  Request to modify the design maximum discharge temperature exit the after Cooler to be 50°C (based on maximum ambient temperature of 40°C). | Agreed. However, it is the responsibility of the bidder to ensure that the efficiencies of succeeding stages / processes are met. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | Vol no. II Process Design Basis.  Pg no. 75,76 clause no. 3, 4 and 5. | **3. Gas Handling capacity**= 0.440 MMSCMD = 4, 40, 000 SCMD.  **4.Compressor Duty:**  LP Compressor  Type 1 =5600 NM3/hr  Type 2 = 2700 NM3/hr  GL Gas compressor  = 3200 NM3/hr  **5. Compressor Utilization:**  LP Compressor – 3 running  GL compressor – 3 running | With 3 compressors running only the type 1 LP compressor can meet the total capacity of 0.440 MMSCMD. Type 2 LP compressor and GL compressor cannot handle the capacity.  Clarity is required for deployment of LP and GL compressors (running and standby) for handling the total quantity of 4,40,000 SCMD gas. | 1. Type 1 X 1 No.  2. Type 2 X 2 Nos.  3. GL Compressor X 3 Nos. |
| 4. | Vol II Technical Part 2  Safety and security during erection. Clause no 3.6.2  Pg. 244 | The LSTK contractor shall comply with BIS : 7205 for necessary safety and adhere to safe erection practices and guard against………. | For Security during erection request OIL to provide CISF personnel with or without payment from the contractor. | It shall be in the scope of the successful bidder. |
| 5. | Page no.36, clause no.8.9 | **Service Tax:**  The price excludes Service Tax and the Service Tax as applicable shall be to the company’s account. The Service Tax amount.........................  .......................................................................................................... Act. | Whether whole contract can be considered as `Works Contract’ under sec 65 (105) clause - zzzza of Service Tax Act and Service Tax can be charged accordingly under Works Contract Service. | Under composite Contract, Service Tax will be applicable on the total contract value.  Works Contract Service Tax will be 40% of Total Contract value X Applicable Rate (15%) |
| 6. | Page no.74, clause no.59(a) | **Central Sales Tax**:  The Contractor shall pay and bear any Central Sales Tax payable in India on the Inter-State Sale of................................... commerce. | Whether OIL can issue required Road Permit and `C’ Form in the name of consignor for purchasing of material in the course of inter-state trade or commerce under E1 sale. | For issuance of road permit & “C”Form, consignment shall be in OIL`s name and in case of “C” Form, the Contractor to submit the Tax Invoice. |