FORM-B

Certificate of Operation at No Load and Lower Load

This is to confirm the following:

1. The offered Gas Engine Generator Model--------------------- Manufactured by ------------------------- is capable of Running at **No Load** (i.e., GEG Breaker Open) for a **minimum period of 30 minutes**, at site conditions (40 deg C ambient temperature, 50% relative Humidity) and utilising Gas fuel of composition as specified in Table – 1, 2 & 3, of the technical specifications.
2. The offered Gas Engine Generator Model-------------------- Manufactured by ------------------------- is capable of **Running continuously** with an Electrical load of **no more than 20% of its Rated capacity (Gross)** as declared in Form-A, Sl. No. 3, at site condition and utilising Gas fuel of composition as specified in Table – 1 of the technical specifications, for a **minimum period of 24 Hours**.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

OEM Authorised Signature Bidder’s Authorised Signature

Company Seal Company Seal